Dalībvalstu iesniegumu apkopojums muitas tarifu atbrīvojumiem vai kvotu piemērošanai
(no 2027.gada 1.jūlija)

Kvotas


	KN kods
	Darba numurs
	Preces apraksts
	Kvotas daudzums

	2849 90 90
	0601
	Zirconium carbide (CAS RN 12070-14-3), with a particle size of 2 μm or more but not more than 7 μm
	Q/14950kilograms, 01.07-31.12

	2921 44 00
	0602
	4-Hydroxydiphenylamine (CAS RN 122-37-2)
	Q/10000kilograms, 01.07-31.12

	2933 39 99
	0603
	2-[3,5-Bis(trifluoromethyl)phenyl]-N-[6-chloro-4-(4-fluoro-2-methylphenyl)pyridin-3-yl]-N,2-dimethylpropanamide (CAS RN 825643-73-0) with a purity of 90 % or more
	Q/30000kilograms, 01.07-31.12

	3204 17 00
	0604
	C.I. Pigment Yellow 120 (CAS RN 29920-31-8) and preparations containing 50 % or more by weight of C.I. Pigment Yellow 120
	Q/5000kilograms, 01.07-31.12

	3815 11 00
	0605
	Components of a catalyst system consisting of at least one of the following:
· nickel oxide and tungsten oxide supported on aluminium oxide, 
· nickel oxide and tungsten oxide supported on silica-alumina, 
· nickel oxide and tungsten oxide supported on a zeolite-based carrier, 
· nickel and tungsten compounds supported on one or more carriers containing at least one of the following: aluminum oxide, silica, and zeolite
	Q/750000kilograms, 01.07-31.12

	3907 29 20
	0606
	Polyether Polyol compromising succrose starters modified with sorbitol, DEG and palm oil as a mixture by weight of;
· Propoxylated succrose 50 % or more but not more than 70 % (CAS RN 9049-71-2)
· Propoxylated sorbitol 5 % or more but not more than 15 % (CAS RN 52625-13-5)
· Propoxylated DEG 10 % or more but not more than 20 % (CAS RN 9051-51-8)
· Propoxylated Palm Oil 10 % or more but not more than 15 % (CAS RN 512802-65-2)
· Water 0,01 % or more but not more than 0,15 % (CAS RN 7732-18-5)
with a hydroxyl number of 410 or more but not more than 460 according to ASTM 4272 method and a viscosity index of 4 000 or more but not more than 7 000 mPas@25C according to ASTM D 4878 method
	Q/29856000kilograms, 01.07-31.12

	3912 20 19
	0607
	Nitrocellulose (CAS RN 9004-70-0) :
· Damped or wetted with water,
· With a nitrocellulose content by weight of 60 % or more,
With a nitrogen  (CAS RN 7727-37-9) content by weight of 12.3 % or more
	Q/400tonnes, 01.07-31.12

	7616 99 10
	0608
	Aluminium alloy Die-cast structural components for motor vehicle rear-view mirror systems or camera monitoring systems:
· for connecting the mirror or camera housing to the vehicle body, weighing 35 grams or more, but not more than 583 grams, or
· for forming the structural frame of the mirror or camera housing, weighing of 81 grams or more, but not more than 1243 grams, or
· for enabling rotational movement of components about an axis of symmetry, weighing 8 grams or more, but not more than 275 grams 
of a kind used in the manufacture of goods of Chapter 87
(1)
	Q/1693356pieces, 01.07-31.12




Muitas nodokļa atcelšana

	KN kods
	Darba numurs
	Preces apraksts

	1515 30 90
	0200
	Castor oil, First Special Grade (FSG), for the manufacture of 11-aminoundecanoic acid and other resulting materials

	2842 90 20
	0401
	Lithium Iron Phosphate, powder used for rechargeable lithium-ion batteries, CAS 15365-14-7
· without carbon, particle size D50 µm 1.0 +/- 1.0, 
· specific surface area (BET) from 7 m2/g to 18 m2/g, 
· tap density from 1 g/cm3 to 2g/cm3, specific discharge capacity from 150 mAh/g to 163 mAh/g and initial efficiency from 94 % to 100 %

	2904 99 00
	0001
	Trifluoromethanesulfonic anhydride (CAS RN 358-23-6) with a purity by weight of 99 % or more

	2909 19 90
	0002
	Isobutyl vinyl ether (CAS RN 109-53-5) with a purity by weight of 97 % or more

	2909 30 90
	0003
	4,4'(chloro(phenyl)methylene)bis(methoxybenzene) (CAS RN 40615-36-9) with a purity by weight of 98 % or more

	2924 19 00
	0004
	17-Amino-10-oxo-3,6,12,15-tetraoxa-9-azaheptadecanoic acid (CAS RN 1143516-05-5) with a purity by weight of 99 % or more

	2924 29 70
	0005
	Anthranilamide of a purity by weight of 99.5 % or more (CAS RN 88-68-6)

	2925 19 95
	0006
	3-Bromopiperidine-2,6-dione (CAS RN 62595-74-8) with a purity by weight of 99 % or more

	2926 90 70
	0007
	2-cyanoethyl N,N,N',N'-tetrapropan-2-ylphosphorodiamidoite (CAS RN 102691-36-1) with a purity by weight of 98 % or more

	2928 00 90
	0008
	2-[2-(1-Cyano-1-methyl-ethyl)hydrazino]-2-methyl-propanenitrile (CAS RN 6869-07-4) with a purity by weight of 98 % or more

	2930 90 95
	0009
	Methyl mercaptoacetate (CAS RN 2365-48-2) with a purity by weight of 98 % or more

	2931 90 00
	0010
	4-(methoxycarbonylphenyl)boronic acid (CAS RN 99768-12-4) with a purity by weight of 99 % or more

	2932 99 00
	0011
	(3-bromo-2,5-dichloro-phenyl)-oxetan-3-yl methanone (CAS RN 2758651-47-5) with a purity by weight of 97 % or more

	2933 19 90
	0012
	Bixafen (CAS RN 581809-46-3) with a purity by weight of 98 % or more

	2933 39 99
	0013
	4-Piperidinemethanol (CAS RN 6457-49-4) with a purity by weight of 98 % or more

	2933 39 99
	0014
	6-Bromopyridin-2-amine (CAS RN 19798-81-3) with a purity by weight of 98 % or more

	2933 39 99
	0015
	Diflufenican (CAS RN 83164-33-4) with a purity by weight of 97 % or more

	2933 59 95
	0016
	2-(Trifluoromethyl)-4H,5H,6H,7H-pyrazolo[1,5-a]pyrazin-4-one (CAS RN 1196153-16-8) with a purity by weight of 98 % or more

	2933 99 80
	0017
	Methyl (2R)-2-amino-3-(7-methyl-1H-indazol-5-yl)propanoate dihydrochloride (CAS RN 1414976-14-9) with a purity by weight of 98 % or more

	2933 99 80
	0018
	5-Nitro-1,3-dihydro-2H-benzimidazol-2-one (CAS RN 93-84-5) with a purity of 91 % by weight or more, in an aqueous suspension

	2934 10 00
	0019
	(2Z)-{2-[(tert-Butoxycarbonyl)amino]-1,3-thiazol-4-yl}{[(1-tert-butoxy-2-methyl-1-oxopropan-2-yl)oxy]imino}acetic acid (CAS RN 137088-65-4) with a purity by weight of 97 % or more

	2934 99 90
	0020
	Ascomycin (CAS RN 104987-12-4) with a purity by weight of 95 % or more

	2934 99 90
	0021
	Wet paste or powder,   
• with a content by weight of 1-{[(6R,7R)-7-amino-2-carboxy-8-oxo-5-thia-1-azabicyclo[4.2.0]oct-2-en-3-yl]methyl}-1-methylpyrrolidin-1-iumchloride (CAS RN 103121-85-3) of 78 % or more, 
• with a content by weight of water of not more than 20 %,   
• and with a dry weight purity of 1-{[(6R,7R)-7-amino-2-carboxy-8-oxo-5-thia-1-azabicyclo[4.2.0]oct-2-en-3-yl]methyl}-1-methylpyrrolidin-1-iumchloride (CAS RN 103121-85-3) of 97 % or more

	2934 99 90
	0022
	N-(1-((2R,3R,4R,5R)-3-fluoro-4-hydroxy-5-(hydroxymethyl)tetrahydrofuran-2-yl)-2-oxo-1,2-dihydropyrimidin-4-yl)acetamide (CAS RN 159414-97-8) with a purity by weight of 98 % or more

	2934 99 90
	0023
	N-(9-((2R,3R,4R,5R)-3-fluoro-4-hydroxy-5-(hydroxymethyl)tetrahydrofuran-2-yl)-9H-purin-6-yl)benzamide (CAS RN 136834-20-3) with a purity by weight of 98 % or more

	3204 11 00
	0201
	Colourant C.I. Disperse Yellow 241 (CAS RN 83249-52-9) and preparations based thereon with a colourant C.I. Disperse Yellow 241 content of 80 % or more by weight 

	3204 19 00
	0202
	Colourant C.I. Solvent Brown 53 (CAS RN 64696-98-6 ) and preparations based thereon with a colourant C.I. Solvent Brown 53 content of 90 % or more by weight 

	3204 19 00
	0203
	Colourant C.I. Solvent Red 195 (CAS RN 72968-71-9) and preparations based thereon with a colourant C.I. Solvent Red 195 content of 80 % or more by weight

	3204 20 00
	0204
	Colourant C.I. Fluorescent Brightener 378 (CAS RN 40470-68-6) and preparations based thereon with a colourant C.I. Fluorescent Brightener 378 content of 70 % or more by weight

	3824 99 96
	0402
	Lithium Iron Phosphate, powder used for rechargeable lithium-ion batteries, 
· mixture with carbon, particle size D50 1.0 µm +/- 1.0, 
· lithium iron phosphate >93 % CAS RN 15365-14-7
· carbon <7 % CAS RN 7440-44-0;
· specific surface area (BET) from 7 m2/g to 18 m2/g, 
· tap density from 1 g/cm3 to 2g/cm3, specific discharge capacity from 150 mAh/g to 163 mAh/g and initial efficiency from 94 % to 100 %

	3901 10 10
	0205
	Uncoloured virgin linear low-density polyethylene (LLDPE) (1-butene/ethylene copolymer) with CAS RN. 25087-34-7, in a form other than powder or flakes:
· having a melt flow index (MFI) (190°C; 2,16 kg) of 1,2 g/10 min or more, but not exceeding 4,5 g/10 min, in accordance with ISO 1133 or ASTM D1238;
· having a density of 0,909 g/cm³ or more, but not exceeding 0,929 g/cm³, in accordance with ISO 1183, ASTM D1505 or ASTM D792;
· having a melting point of 89°C or higher, but not higher than 136°C, determined by differential scanning calorimetry;
· containing slip additives (SLIP) not exceeding 50 ppm;
· containing anti-blocking agents not exceeding 50 ppm;
· containing antioxidants exceeding 1 ppm;
· having a haze (HAZE) level below 35 %, in accordance with ASTM D1003;
· produced from monomers not derived from coal, chemical recycling, or renewable sources;
· manufactured using gas-phase or solution (liquid-phase) processes with Ziegler–Natta and metallocene type catalysts;
· not containing carbon black

	3920 99 28
	0206
	Thermoplastic polyurethane foil in rolls, with:
· a width of 475 mm or more, but not more than 1060 mm,
· a matt finish,
· a thickness 0,35 mm or more, but not more than of 0,4 mm (± 8 %),  
· an elongation at break of 400 % or more (ASTM D412 (Die C)),
· a tensile strength in machine direction of 40 MPa or more,
· a Shore A hardness of 90 (± 3) (ASTM D2240),
· a tear strength of 100 (± 10)  kg/cm²  (ASTM D624 (Die C)),
· a melting point of 165°C (± 10 °C)  

	7616 99 90
	0403
	Spigot - Deep-drawn aluminium connector for battery coolers of electric motor vehicles:
· with a height of 10 mm or more but not more than 25 mm,
· with a diameter of 15 mm or more but not more than 30 mm,
made of EN AW-3003 aluminium alloy composition according to DIN EN 573-3.

	8411 99 00
	0404
	Turbine component ("S-vane") for use in variable turbine geometry (VTG) turbochargers, with a wave profile and tapered end, made of alloy steel, with:
· a heat-resistance of not more than 1050 °C;
· an overall length of at least 15 mm but not more than 25 mm;
a height of s-vane portion at least 3 mm but not more than 9 mm

	8419 50 80
	0405
	Forgó-type, water-to-air, aluminium, mechanical tube-rib connection heat exchanger (aluminium Forgo-bundle):
· with fin thickness of at least 0.18 mm but not more than 0.28 mm
· with fin pitch of at least 2.8 mm but not more than 4.25 mm
· with tube diameter of at least 15 mm but not more than 30 mm

	8481 80 59
	0406
	Electronic air intake control module for regulating the amount of air supplied to a spark-ignition internal combustion engine, consisting of:
· an integrated air duct,
· an electronically controlled throttle valve,
· an electric motor,
· position and pressure sensors,
for use in the manufacture of internal combustion engines for motor vehicles (1)

	8481 80 99
	0407
	Integrated thermal management module for controlling the flow of coolant, consisting of an electrically operated three-way valve, an electric motor and connection nipples,
for use in the manufacture of internal combustion engines for motor vehicles (1)

	8482 10 90
	0408
	Deep-groove ball bearing, for use in a single-speed or two-speed transfer case:
· manufactured from 100Cr6 /1.3505 (EN/DIN) steel,
· an external diameter of 52 mm or more but not more than 100 mm,
a width of 5 mm or more but not more than 28 mm.

	8482 40 00
	0409
	Drawn cup needle roller bearing, for incorporation into a two-speed transfer case:
· with rolling elements made of GCr15 / 100Cr6 steel,
· a drawn cup made of SAE 1010 steel,
· a cage made of PA66-GF30 plastic,
· an external diameter of 86 mm or more but not more than 106 mm,
a width of 5 mm or more but not more than 22 mm

	8501 51 00
	0410
	Two-bearing, brushless AC motor with:  
· an external motor housing diameter of 91 mm or more, but not more than 94 mm, 
· three phase or six phase windings, 
· a rated voltage of 12 V, 
· a maximum mechanical power at rated voltage of 630 W or more, but not more than 1 570 W, 
· a rated speed of 1 238 rpm or more, but not more than 1 514 rpm, 
· a peak current of 72 A or more, but not more than 88A, 
· permanent magnets of the surface or interior type, 
· a pulley, 
· a single phase resistance of 4,9327 mΩ or more, but not more than 7,5819 mΩ at an operating temperature of 20 °C, 
· a maximum torque constant of 34,8386 mNm/A or more, but not more than 48,7099 mNm/A at 20 °C, 
· inductance not exceeding 46,451mH on the d axis and not exceeding 49,0560 mH on the q axis, 
· a back electromotive force constant (Ke) of 0,0402 V·s/rad or more, but not more than 0,0590 V·s/rad,
· a motor constant (Km) of 0,0074 or more, but not more than 0,0120 Nm/A/√Ω, 
· a mechanical time constant of 0,2994 ms or more, but not more than 0,5236 ms, 
· a torque of 6,79 Nm or more, but not more than 10,34 Nm, 
· even equipped with a rotor position sensor of the dipole magnet type, 
· an electronic star-point relay,  
· 12-slots stator, 
8-pole rotor

	8503 00 98
	0411
	Electric motor rotor shaft with internal involute splines, external screw threads and at least two holes, for use in the manufacture of electric drives for motor vehicles (1)

	8505 90 90
	0412
	Electromagnetic coil:
· consisting of a cylindrical steel yoke ring, a steel cover, a plastic bobbin, a copper wire winding with insulating lacquer coating, a stainless steel spring plate and 2 or 3 copper alloy terminal contacts; 
· including a central through bore,
· with an outer diameter of the assembly of 17.4 mm or more but not more than 23.9 mm, a central bore diameter of 9.2 mm or more but not more than 11.3 mm, and an axial length of 20.1 mm or more but not more than 21.8 mm.
· with a net weight of 13.8 g or more but not more than 31.3 g;
containing no plunger or other movable actuators

	8512 20 00
	0413
	Passenger vehicle lamp LED PCBAs (Printed Circuit Board Assemblies):
· with LED components,
· with thickness of 1,44 or more, but not more than 1,76 mm,
· with width of 25 mm or more, but not more than 90 mm,
· with length of 150 mm or more, but not more than 330 mm,
· a weight of 10g or more, but not more than 60g,
· PCB material – including FR-4 (Flame Retardant 4),
· containing two PCB layers,
· copper plate thickness of 35 µm, 
surface treatment: OSP (Organic Solderability Preservative)

	8516 80 80
	0414
	High-voltage electric heating resistor (element) based on PTC thermistors:
· composed predominantly of aluminum electrodes and ceramic PTC elements,
· provided with a sheath of high-temperature electrical insulation based on polymer film,
· designed for a high operating DC voltage in the range of 100 V to 600 V (with a rated voltage in the range of 200 V to 450 V),
· with a steady-state electrical current in the range of 1.0 A to 6.0 A (depending on rated voltage and configuration),
· with a maximum in-rush current not exceeding 15 A,
· having a total heating element length of 220 mm or greater, but not exceeding 280 mm,
· with a total mass not exceeding 150 g,
· with a maximum heating element surface temperature not exceeding 230 °C,
· designed for an ambient operating temperature range from -40 °C to +110 °C,
without integrated control electronics, with electrical connection via crimped copper or brass terminals

	8516 80 80
	0415
	Electric heating resistor (element) based on PTC thermistors:
· composed predominantly of an aluminum heat sink and ceramic PTC elements,
· with mounting and insulating components made of glass fiber-reinforced engineering plastics,
· designed for an operating DC voltage in the range of 9 V to 52 V (rated voltage 13 V or 44 V),
· with a steady-state electrical current in the range of 18 A to 67 A (depending on rated voltage and internal configuration),
· with a maximum in-rush current not exceeding 70 A,
· having a total heating element length of 168 mm or greater, but not exceeding 202 mm,
· with a total mass not exceeding 80 g,
· with a maximum aluminum fin surface temperature not exceeding 185 °C,
· designed for an ambient operating temperature range from -40 °C to +110 °C,
without integrated control electronics, with electrical connection via blade terminals

	8537 10 98
	0416
	Rotary and push-button control unit for operating a vehicle audio and navigation system, comprising:
· a rotary knob with a push-button function,
· a printed circuit board with an integrated circuit,
· with or without cable with a connector
for use in the manufacture of goods of Chapter 87 (1)


	8537 10 98
	0417
	Parking brake latch control unit in assembly with actuator, comprising:
· a brushless DC electric motor,
· a printed circuit board,
· position sensors,
· a reduction gear mechanism with output shaft,
· housing,
· a connector
for use in the manufacture of electric drives for motor vehicles (1)

	8708 50 35
	0418
	Drive-axle, for incorporation into the transfer case for motor vehicles:
· made of SCM420H steel,
· with an external diameter of 37 mm or more but not more than 87 mm,
with a length of 285 mm or more but not more than 320 mm

	8708 50 99
	0419
	Two-speed transfer case cover:
· made from EN AC-46000/AlSi9Cu3(Fe) aluminium alloy casting,
· a length of 285 mm or more but not more than 440 mm,
· a width of 250 mm or more but not more than 280 mm,
a height of 85 mm or more but not more than 185 mm

	8708 50 99
	0420
	Two-speed transfer case housing:
· manufactured from EN AC-46000/AlSi9Cu3(Fe) aluminium alloy,
· a length of 420 mm or more but not more than 440 mm,
· a width of 280 mm or more but not more than 300 mm,
a height of 95 mm or more but not more than 115 mm.

	8708 94 91
	0421
	Inner support bracket made of SAE J403 grade 1010-1020 steel (of modified chemistry for carbon content of no more than 0,12) with:
· material thickness of 5,24 mm or more, but not more than 5,76 mm,
· rivets pads profile of not more than 0,2 mm related to datum,
· rivets hole diameter of 7,15 mm or more, but not more than 7,25 mm, 
· rivets sliding pads flatness of not more than 0,25 mm,
· rivets sliding inside width of 7,15 mm or more, but not more than 7,25 mm,
· mounting hole size of 9,95 mm or more, but not more than 10,05 mm,
· cathodic e-coat thickness of 0,015 mm or more, but not more than 0,025 mm,
· without burrs around entire opening, top and bottom rivets sliding slot

	8708 94 99
	0422
	Column mounting bracket made of die-casted magnesium per ASTM B94 grade AM50A with: 
· a draft angle of not more than 2 degrees,
· a through-bolt mounting hole diameter of 8,1 mm or more, but not more than 8,15 mm,
· a wire harness locating feature width of 6 mm or more, but not more than 6,4 mm,
· a clip interface thickness of 2,8 mm or more, but not more than 3,2 mm,
· a clip interface slot length of 6,7 mm or more, but not more than 6,9 mm,
· a clip interface slot width of 5,7 mm or more, but not more than 5,9 mm,
· a cross car beam mounting alignment features profile tolerance of not more than 0,5 mm related to datums ABC,
· a bracket ear width of 9,9 mm or more, but not more than 10,1 mm

	8708 94 99
	0423
	Rake bracket assembly welded parts, consisting of a rake bracket and a rake upper bracket, made of GB/T 711 grade 08 steel or BG Z J565-2015 SPHC to Q/BQB 302, with:
· a rake upper bracket material thickness of 3,25 mm or more, but not more than 3,59 mm,
· a rake bracket material thickness of 2,85 mm or more, but not more than 3,15 mm,
· a slot width of 9,17 mm or more, but not more than 9,37 mm,
· a width of welded left and right brackets true position of not more than 0,5 mm related to datums ABC,
· a width of welded left and right brackets of 60,3 mm or more, but not more than 61,0 mm,
· a minimum axial load at two points simultaneously of 7 kN without weld fracture,
· capsules edge around profile of not more than 0,25 mm

	8708 94 99
	0424
	Compression or rake bracket assembly, made of SAE J403 grade 1020 steel or of SAE J403 Grade 1010-1020 steel (of modified chemistry for carbon content of 0,18 or more, but not more than 0,22), comprising one or more brackets (including inner and outer or left and right elements), with:
· an element material thicknesses of 1,85 mm or more, but not more than 5,65 mm
· an entire tooth profile of no more than 0,3 mm related to datums ABC,
· a maximum axial load of 10 kN or more without weld fracture,
· with or without a mounting plate: 
· incorporating 3 holes for rivets with a diameter of 6,8 mm or more but not more than 6,9 mm,
continous surface of top surface formed by die roll and direction punch

	8708 94 99
	0425
	Lower jacket made of EN10305-2 grade E235+C or S235JR per Q/BQB 303 with:
· assist mechanism plate made of SAE J403 grade 1008-1010 steel or S420MC per Q/BQB311,
· assist mechanism plate material thickness of 4,9 mm or more, but not more than 5,1 mm,
· an inner diameter of 37,43 mm or more, but not more than 37,59 mm,
· an outer diameter of 40,02 mm or more, but not more than 40,16 mm,
· an outer diameter straightness of not more than 0,25 mm,
· assist mechanism plate machined contact surface runout of not more than 0,1 mm related to datum A,
· a total length of 172,63 mm or more, but not more than 173,13 mm,
a bottom edge perpendicularity of not more than 0,08 mm related to datum A

	ex 1902 30 10
	0301
	Glass noodles containing 60 % or more by weight of mung bean starch in immediate packings of 5 kg or more and not put up for retail sale

	ex 2106 90 92
ex 3504 00 90
	0302
	Casein protein hydrolysate consisting of:
· by weight 20 % or more but not more than 70 % free amino acids, and
peptones of which by weight more than 90 % having a molecular weight of not more than 2000 Da

	ex 3919 10 80
ex 3919 90 80
ex 3920 61 00
	0305
	Reflecting sheet:
·  of a polycarbonate or acrylic polymer film embossed on one side in a regular shaped pattern
·  covered on one or both sides with one or more layers of plastic or metallisation, and
whether or not covered on one side with a self-adhesive layer and a release sheet

	7410 21 00
	0307
	Plates:
· consisting of at least one layer of fibreglass fabric impregnated with epoxide resin,
· covered on one or both sides with copper foil with a thickness of not more than 0,15 mm,
· with a dielectric constant (DK) of less than 5,4  at 1 MHz, as measured according to IPC-TM-650 2.5.5.2,
· with a loss tangent of less than 0,035 at 1 MHz, as measured according to IPC-TM-650 2.5.5.2,
with a comparative tracking index (CTI) of 600 or more




Dalībva lstu iesniegumu apkopojums muitas tarifu   atbrīvojumi em vai kvotu piemērošanai   (no 2027.gada 1.jūlija)     Kvotas      

KN kods  Darba  numurs  Preces apraksts  Kvotas daudzums  

2849 90 90  0601  Zirconium carbide (CAS RN 12070 - 14 - 3), with a particle size of 2 μm   or more but not more than 7 μm  Q/14950kilograms, 01.07 - 31.12  

2921 44 00  0602  4 - Hydroxydiphenylamine (CAS RN 122 - 37 - 2)  Q/10000kilograms, 01.07 - 31.12  

2933 39 99  0603  2 - [3,5 - Bis(trifluoromethyl)phenyl] - N - [6 - chloro - 4 - (4 - fluoro - 2 - methylphenyl)pyridin - 3 - yl] - N,2 - dimethylpropanamide (CAS RN 825643 - 73 - 0) with a purity of 90   % or more  Q/30000kilograms, 01.07 - 31.12  

3204 17 00  0604  C.I. Pigment Yellow 120 (CAS RN 29920 - 31 - 8) and preparations containing 50   % or more by weight of C.I. Pigment Yellow 120  Q/5000kilograms, 01.07 - 31.12  

3815 11 00  0605  Components of a catalyst system consisting of at least one of the following:   -   nickel oxide and tungsten oxide supported on aluminium oxide,     -   nickel oxide and tungsten oxide supported on silica - alumina,     -   nickel oxide and tungsten oxide supported on a zeolite - based carrier,     -   nickel and tungsten compounds supported on one or more carriers containing at least one of the following: aluminum oxide, sil ica, and  zeolite  Q/750000kilograms, 01.07 - 31.12  

3907 29 20  0606  Polyether Polyol compromising succrose starters modified with sorbitol, DEG and palm oil as a mixture by weight of;   -   Propoxylated succrose 50   % or more but not more than 70   % (CAS RN 9049 - 71 - 2)   -   Propoxylated sorbitol 5   % or more but not more than 15   % (CAS RN 52625 - 13 - 5)   -   Propoxylated DEG 10   % or more but not more than 20   % (CAS RN 9051 - 51 - 8)   -   Propoxylated Palm Oil 10   % or more but not more than 15   % (CAS RN 512802 - 65 - 2)   -   Water 0,01   % or more but not more than 0,15   % (CAS RN 7732 - 18 - 5)   with a hydroxyl number of 410 or more but not more than 460 according to ASTM 4272 method and a viscosity index of 4 000 or m ore but  not more than 7 000 mPas@25C according to ASTM D 4878 method  Q/29856000kilograms, 01.07 - 31.12  

3912 20 19  0607  Nitrocellulose (CAS RN 9004 - 70 - 0) :   -   Damped or wetted with water,   -   With a nitrocellulose content by weight   of 60   % or more,   With a nitrogen     (CAS RN 7727 - 37 - 9) content by weight of 12.3   % or more  Q/400tonnes, 01.07 - 31.12  

